* A dynamic model for the modelling of parabolic through collectors is proposed
* A steady-state and dynamic validation against data from the PSA faciity is presented
* Simulation results shown good accuracy with experimental data
* A discretization level of 20 CV is found to be optimal between model accuracy and simulation speed
* A 1 CV collector model is proposed for daily or longer time frame